{"text_format":"3","workbook":"xls","n_sheets":3,"sheets":["Sheet1","Sheet2","Sheet3"],"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Sheet1","index":0,"n_rows":13,"n_cols":7,"rows_kept":13,"merged":[[0,0,0,6],[1,0,2,0],[1,1,2,1],[1,2,2,2],[1,3,2,3],[1,4,2,4],[1,5,2,5],[1,6,2,6],[3,0,9,0],[10,0,12,0]],"flags":["formulas_cached_only"]}
["淖尔壕煤矿物资采购明细表"]
["包号","序号","设备、器材名称","型号及规格","单位","数量","备注"]
[]
["包\n一","一","箱式变电站"]
[null,1,"高压开关柜","XGNG-12","台",3,"详见图纸及技术要求"]
[null,2,"低压开关柜","GGD型  380V","台",6,"详见图纸及技术要求"]
[null,3,"低压开关柜","GGD型  660V","台",3,"详见图纸及技术要求"]
[null,"4","变压器","SB10-1250/10/0.4KV","台",1,"详见图纸及技术要求"]
[null,"5","变压器","SB10-1000/10/0.69KV","台",1,"详见图纸及技术要求"]
[null,"6","箱体",null,"套",1,"详见图纸及技术要求"]
["包\n二","二","卧式离心泵"]
[null,1,"卧式离心泵","流量360m3/h,扬程70M","台",3]
[null,2,"配套软启动控制柜","满足水泵电机功率要求并可接自动控制","台",3]

{"sheet":"Sheet2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}

{"sheet":"Sheet3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}