{"text_format":"3","workbook":"xls","n_sheets":3,"sheets":["Sheet1","Sheet2","Sheet3"],"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Sheet1","index":0,"n_rows":9,"n_cols":6,"rows_kept":9,"merged":[[0,0,0,5],[1,0,1,1],[1,2,1,5],[2,1,2,2],[8,0,8,5]],"flags":["formulas_cached_only"]}
["两台主通风机防腐除锈工程量明细"]
["风机型号 ",null,"FBCDZ-10-No.29(B)"]
["序号","维修内容",null,"单位","数量","备注"]
[1,"消音设施","扩散塔内消音棉填充、消音网更换、修补","台",2,"工程量现场核对"]
[2,"防腐除锈","两台风机内部、外部防腐除锈、外部喷原字样、连接筒之间做密封","台",2,"工程量现场核对、字体与原字体规格一样"]
[3,"防结冰排    水管","两台风机内、外管路疏通、排水管做保温","台",2,"清理管道内淤泥及疏通各出水口"]
[4,"蝶阀加热","蝶阀加热伴热带护罩修复","台",2]
[5,"蝶阀阀芯","蝶阀阀芯处漏风","台",2,"现场核对维修工程量"]
[" 生产厂家：山西运城安瑞节能风机有限公司 生产日期：2012年11月20日"]

{"sheet":"Sheet2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}

{"sheet":"Sheet3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}